Uses of Class com.jlrfid.service.RFIDException

Package | Class | Use | Tree | Deprecated | Index | Help

PREV NEXT | FRAMES NO FRAMES

## Uses of Class
com.jlrfid.service.RFIDException

Uses of RFIDException in com.jlrfid.service

Methods in com.jlrfid.service that throw RFIDException
`boolean` | `MainHandler.BeginInv(GetReadData getReadData)` reading circulation when start to circulation reading, do other operation should stop inventory first, such write tag or read antenna send circulation reading order by start sub thread, after sending order, the method will callback function getReadData
`boolean` | `MainHandler.BeginInv(GetReadData getReadData)` reading circulation when start to circulation reading, do other operation should stop inventory first, such write tag or read antenna send circulation reading order by start sub thread, after sending order, the method will callback function getReadData
`boolean` | `MainHandler.InvOnce(GetReadData getReadData)` inventory once send circulation reading order by start sub thread, after sending success, the method will callback getReadData.
`boolean` | `MainHandler.InvOnce(GetReadData getReadData)` inventory once send circulation reading order by start sub thread, after sending success, the method will callback getReadData.
`boolean` | `MainHandler.KillTag(java.lang.String pKill_pwd, java.lang.String access_pwd)` kill tag
`boolean` | `MainHandler.KillTag(java.lang.String pKill_pwd, java.lang.String access_pwd)` kill tag
`boolean` | `MainHandler.lockTag(int opcode, int block, java.lang.String password)` lock tag
`boolean` | `MainHandler.lockTag(int opcode, int block, java.lang.String password)` lock tag
`static void` | `OnecReadDemo.main(java.lang.String[] args)`
`static void` | `LoopReadDemo.main(java.lang.String[] args)`
`java.lang.String` | `MainHandler.ReadTagData(int bank, int begin, int size, java.lang.String password)` get the single card data, can set the reading area, start address and reading length
`java.lang.String` | `MainHandler.ReadTagData(int bank, int begin, int size, java.lang.String password)` get the single card data, can set the reading area, start address and reading length
`boolean` | `MainHandler.SetAlive(byte intervalSecond)` set alive time interval
`boolean` | `MainHandler.SetAlive(byte intervalSecond)` set alive time interval
`boolean` | `MainHandler.SetAnt(byte[] antEnable, long[] dwellTime, long[] power)`
`boolean` | `MainHandler.SetAnt(byte[] antEnable, long[] dwellTime, long[] power)`
`boolean` | `MainHandler.SetDO(byte port, byte state)` set Digital Output status
`boolean` | `MainHandler.SetDO(byte port, byte state)` set Digital Output status
`void` | `Demo.testLockTag()`
`void` | `Demo.testReadCard()`
`void` | `Demo.testSetAlive()`
`void` | `Demo.testSetAnt()`
`void` | `Demo.testSetDO()`
`void` | `Demo.testStopInv()`
`void` | `Demo.testWriteCard()`
`boolean` | `MainHandler.WriteTagData(char bank, char begin, char size, java.lang.String data, java.lang.String password)` write single card data, can set the writing area, start add and reading length
`boolean` | `MainHandler.WriteTagData(char bank, char begin, char size, java.lang.String data, java.lang.String password)` write single card data, can set the writing area, start add and reading length

Package | Class | Use | Tree | Deprecated | Index | Help

PREV NEXT | FRAMES NO FRAMES